Lab1; introduction to Networking with Wireshark

*Request legorafi.fr by mobile phone*

No Time Source Destination Protocol Length Info

9791 302.301362 192.168.43.35 78.109.84.17 HTTP 410 GET / HTTP/1.1

Ethernet source address: 80:86:f2:b2:65:fb

Ethernet destination address: c0:ee:fb:46:a0:2c

IP source address: 192.168.43.35

IP destination address: 78.109.84.17

Transmission protocol : TCP

With ipconfig /all

Machine physical address : 80-86-f2-b2-65-fb

Ip address (ipv4) : 192.168.43.35

The destination correspond to one of the gorafi serveurs to which we ask the data.