VLAN; class 3

orange means “blocked”. All led of switches are orange by defualts.